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	SAFE WORK METHOD STATEMENT

	
	BNP SWMS 08 - StreetBond V2
	Issued 15-May-25

	ABN:  69 056 378 575
	ACN: 056 378 575
	11 Huntington Place, Banyo QLD 4014
	PH: (07) 3630 2500
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	Location
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	Person in control of works
	     
	Contact Number
	     

	Work Activity
	Applying StreetBond

	High Risk Construction Activities
	[bookmark: Check1]|_| Risk of a person falling more than 2 metres
	[bookmark: Check2]|_| Work in or near a confined space
	[bookmark: Check3]|_| Work in or near a shaft or trench deeper than 1.5 m or a tunnel

	
	[bookmark: Check4]|_| Work on or near pressurised gas mains or piping
	[bookmark: Check5]|_| Work on or near energised electrical installations or services
	[bookmark: Check6]|X| Work on, in or adjacent to a road, railway, shipping lane or other traffic corridor in use by traffic other than pedestrians

	
	[bookmark: Check7]|_| Work in an area with movement of powered mobile plant
	[bookmark: Check8]|_| Work in or near water or other liquid that involves a risk of drowning
	[bookmark: Check9]|_| Is carried out in an area that may have a contaminated or flammable atmosphere

	Consultation in development of SWMS
	Name
	Position
	Signature
	Date

	
	Greg Steele
	Director
	[image: ]
	[bookmark: Text5]     

	
	Brendan Evans
	QLD Manager
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	Approved by
	Brendan Evans
	Position
	QLD Manager
	Signature
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	Date
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	Legislation and Codes of Practice
	Work Health & Safety Act 2011, Work Health & Safety Regulation 2011, How to Manage Work Health and Safety Risks COP 2011, Work Health and Safety Consultation, Co-operation and Co-ordination 2011
Traffic Management for Construction or Maintenance Work Code of Practice 2008, MUTCD Part 3
Managing the Risks of Hazardous Chemicals Code of Practice 2021, Hazardous Manual Tasks Code of Practice 2021, Managing Risks of Plant Code of Practice 2021, Abrasive Blasting Code of Practice 2021, First Aid in the Workplace Code of Practice 2021

	Plant and Equipment required
	Mixer, air compressor, paint gun.

	Inspections and maintenance
	Preoperational check to be conducted on plant

	Materials used
	StreetBond Coating

	Specific Training
	General industry induction (QLD white card); Site specific induction, trained in SWMS / SDS procedures, Trained in Safe & Proper Use of PPE

	Personal Protective Equipment
	Mandatory PPE to be worn at all times – Hi-Vis Long Sleeve shirt – (Sleeves rolled down) or Hi-Vis vest over shirt, Long pants, Safety glasses, gloves when Manual Handling, Safety helmet where required.
Task PPE – Ears plugs (over 70db), Respirators, Knee high leather chaps



	[bookmark: _Hlk23188243][bookmark: _Hlk23188256]Implement, Monitor and Review

	Actions before work commences
	Workers will be inducted onto the Safe Work Method Statement
Traffic management controls, approved plans and permits must be in place before working within 6mtrs of live traffic.
All traffic controllers must hold the relevant qualification for the role. Evidence must be sighted prior to start of works.
Works must be planned and structured to cause minimum disruption to local traffic, pedestrians and residents.
Conduct pre-operational checks on plant

	Actions during works
	Signage checks must be completed at regular intervals and documented throughout the day.
Works will be monitored to ensure works are carried out in accordance with the Safe Work Method Statement
Report any hazards or incidents.
Person in control of the works is the nominated person who will ensure the implementation of this SWMS.
All incidents and / or near misses must be reported following the Brick N Pave incident reporting process.

	Actions after work is completed
	Safe Work Method Statement will be reviewed and amended when changes are made or where a new hazard has been identified, or at least annually  





	Risk Assessment



	HEALTH & SAFETY CONSEQUENCES
	1. INSIGNIFICANT
- no injuries
	2. MINOR
- first aid treatment, spillage contained on site
	3. MODERATE
- medical treatment, spillage contained with outside help
	4. MAJOR
- extensive injuries, loss of production
	5. CATASTROPHIC
- death, toxic release of chemicals
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	PROBABILITY
	A. Common or Frequent Occurrence
	M5
	M10
	H15
	E20
	E25
	

	
	B. Is known to Occur or ‘It Has Happened”
	L4
	M8
	H12
	E16
	E20
	

	
	C. Could Occur or “I’ve Heard of it Happening”
	L3
	M6
	M9
	H12
	H15
	

	
	D. Not Likely to Occur
	L2
	L4
	M6
	M8
	M10
	

	
	E. Practically Impossible
	L1
	L2
	L3
	L4
	M5
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	Identified Hazards and Control Measures

	Item
	Job sequence
	Potential Hazards
	Risk
	Risk
L x C = R 
	Control Measures
	Residual Risk
L x C = R
	Responsible Person

	
	Site Establishment of works on, in or adjacent to a road or traffic corridor in use by traffic other than pedestrians
	Public
	Incident due to proximity to adjacent road
	
	BNP to hire a licensed Traffic Management Company to develop and establish appropriate traffic management controls taking in consideration sequencing, job specific Temporary Road Closure Approval requirements and scheduling of works.
Ensure permits are current.
Traffic Management Plan and Traffic Guidance Schemes to be developed and implemented by a licenced traffic management company.
Ensure traffic management controls are inspected and signed off by traffic management company.
Site vehicles to have warning devices (e.g., flashing lights, vehicle signage, etc.).
Workers to wear high visibility clothing (night vis as required).
	
	BNP representative
Traffic Management Company

	
	Starting Work
	Poor consultation
	Incident due to poor consultation
	
	BNP to coordinate consultation between site personnel and traffic control company.
Consultation to include 
Scheduling of works
Movement of plant and vehicles
Nominated UHF channel
Specific hazards and controls relevant to the shift
Emergency response
	
	BNP representative


	
	Unloading plant
	Falls
	Injury due to fall
	
	Ensure fall protection is in place on truck.
Utilise ladder access to rear of truck.
	
	BNP representative

	
	
	Manual Tasks
	Sprains and strains
	
	Use mechanical assistance to lift heavy plant for truck.
Ensure personnel understand what manual handling is not just about the weight e.g. for example, twisting, jerking or reaching, doing the task too fast, using too much force or lifting the wrong way.
If mechanical assistance is not reasonable, utilise team lifts.
	
	BNP representative
Site personnel

	
	Marking out area
	Chemical
	Contact with paint
	
	Avoid eye and skin contact.
Wear safety glasses
Wear protective clothing to avoid skin contact
	
	BNP representative
Site personnel

	
	Mixing product
	Chemical
	Contact with StreetBond
	
	Operator to conduct preoperational checks on plant.
Major defects are to be reported to the BNP representative.
Wear respiratory protection when mixing dry product.
Be aware of other workers and proximity to traffic.
	
	BNP representative
Site personnel

	
	Application
	Overspray
	Contact with workers
	
	Determine whether wind conditions may affect other workers or adjacent traffic.
Work is not to distract adjacent traffic.
Conduct a couple of test runs to determine suitability of exclusion zones / direction of work.
Supervisor to monitor progress of works and any change.
	
	BNP representative
Site personnel

	
	General site hazards
	Fuelling Plant
	Contact with fuel
Fire
	
	Ensure correct fuel is used.
Ensure spill kit and ABE fire extinguisher is available.
Ensure no naked flames are in the fuelling area
	
	BNP representative
Site personnel

	
	
	Noise
	Exposure to excessive noise
Hearing Damage
	
	Assess work area for excessive noise.
Generally, if there is a need to shout due to production noise, controls need to be implemented.
When deciding control measure, the hierarchy of control must be considered, and the highest reasonably practicable control measure must be used e.g. remove personnel away from the noise rather than PPE.
	
	BNP representative
Site personnel

	
	
	Dust
	Inhalation of airborne contaminants 
	
	Work activities that produced to be monitored and where possible dust should be controlled by engineering controls such as water suppression or extraction
If dust cannot be controlled that ensure workers are protected by suitable respiratory protection.  
Ensure other workers are removed from the immediate area.
	
	BNP representative
Site personnel

	
	
	Working outdoors
	Heat Stress
Skin Cancer
	
	Personnel to be aware of the signs and symptom of heat illness and provided advice on how to minimise the risk including
Keep hydrated, about 250ml per 30minutes
Monitor yourself
Check in with your mate
Avoid alcohol and caffeine
Signs and symptoms of heat stress include
Pale clammy or hot flushed dry skin
Headaches
Nausea and/or vomiting
Personnel to be protected from the risk of sun damage.  PPE requirements include sunscreen, brims, sunglasses, longs sleeves and long pants.
Personnel to report any symptoms of heat illness to BNP representative immediately.  Personnel to receive first aid and medical attention.
BNP representative to promote heat illness prevention during daily prestart meeting and toolbox meetings.
	
	BNP representative
Site personnel

	
	Finalise Works
	Equipment left on road
Traffic signage not removed / reinstalled
	Incident due to contact with equipment
Inappropriate signage
	
	BNP representative to inspect closed work area to ensure all equipment is accounted for and packed onto the site vehicles.
Liaise with traffic management company before opening work area.
Traffic Management company to establish normal traffic conditions.
BNP representation to conduct a final inspection to ensure
No equipment has been missed
All temporary signage has been removed
All cover traffic signage has been restored 
	
	BNP representative
Traffic Management Company









	Additional Hazards and Control Measures

	Item
	Work Activity
	What can go wrong 
	What will be put in place
	Responsible Person

	1. 
	
	
	
	

	1. 
	
	
	
	

	1. 
	
	
	
	

	1. 
	
	
	
	

	1. 
	
	
	
	







	Name
	Signature
	Date
	Name
	Signature
	Date

	I the undersigned, confirm that the SWMS nominated above has been explained and its contents are clearly understood and accepted.
I confirm that required qualifications to undertake the activity are current.  I clearly understand the controls in this SWMS must be applied as documented, otherwise work is to cease immediately.  I have been provided with the Personnel Protective Equipment identified, consulted and given the opportunity to comment on this SWMS.
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